Guide 1: How to Bleed a Radiator
Why do this?
If your radiator is cold at the top but warm at the bottom, air may be trapped inside.
What you'll need
· Radiator key
· Old towel
· Small container
Steps
1. Turn off your heating.
2. Wait for radiators to cool.
3. Place a towel under the valve.
4. Insert the radiator key.
5. Turn slowly anti-clockwise.
6. Allow trapped air to escape.
7. When water appears, close the valve.
8. Switch heating back on.
Contact MDC if:
· Water leaks continuously.
· The valve is damaged.
· The radiator still won't heat properly.


